<?xml version="1.0" encoding="UTF-8" standalone="no" ?>
<JingJiBiao BiaoDuanNO="11" Jsfs="1" Version="3.2" Xmmc="张家港市垃圾处理场应急飞灰库（北）工程">
<QtXinXi>
<QtXinXiMx Mc="招标代理费" Zhi="0"/>
</QtXinXi>
<ZhaoBiaoXx BzTime="2019-10-30" Bzr="吴芳芳" FhTime="2019-10-30" Fhr="陶有成" Zbr="张家港市市容管理处" ZbrDb="杜凯" Zxr="江苏金港项目管理有限公司" ZxrDb="赵苹"/>
<Dxgcxx Aqwmf="0" Dxgcbh="001" Dxgcmc="张家港市垃圾处理场应急飞灰库（北）工程" Gf="0" Je="0" Zgj="0">
<Dwgcxx DogNum="161618808278" Dwgcbh="001" Dwgcmc="垂直防渗工程" MachineKey="C0:3F:D5:75:B3:09" SoftName="南京未来高新技术有限公司" SoftNum="空" Zylb="4">
<Fywj/>
<Gfsj>
<GfsjMx Fl="100" Fyxlb="1" Je="0" Jsjc="分部分项工程费+措施项目费+其他项目费-除税工程设备费" Mc="规费" Qfjs="0" Xh="1"/>
<GfsjMx Fl="1.3" Fyxlb="1.1" Je="0" Jsjc="分部分项工程费+措施项目费+其他项目费-除税工程设备费" Mc="社会保险费" Qfjs="0" Xh="1.1"/>
<GfsjMx Fl="0.24" Fyxlb="1.2" Je="0" Jsjc="分部分项工程费+措施项目费+其他项目费-除税工程设备费" Mc="住房公积金" Qfjs="0" Xh="1.2"/>
<GfsjMx Fl="9" Fyxlb="2" Je="0" Jsjc="分部分项工程费+措施项目费+其他项目费+规费-(甲供材料费+甲供设备费)" Mc="税金" Qfjs="0" Xh="2"/>
<GfsjMx Fl="100" Fyxlb="3" Je="0" Jsjc="" Mc="合计" Qfjs="0" Xh="3"/>
</Gfsj>
<Qdxm>
<QdBt Bz="" Je="0" Mc="D桩基工程" Xh="1" Zgj="0">
<Qdmx Bz="" Clf="0" Dw="m" Fcf="0" Glf="0" Jsgz="按设计图示尺寸以桩长计算" Jxf="0" Lr="0" Mc="深层水泥搅拌桩" Qdbm="040201013001" Rgf="0" Sbf="0" Sl="10632" Xh="1" Xmtz="1.地层情况:详见设计图纸&#xD;&#xA;2.空桩长度、桩长:空桩长度请踏勘现场，结算不调整。设计桩长21~23m&#xD;&#xA;3.桩截面尺寸:三轴水泥搅拌桩φ650@450mm&#xD;&#xA;4.水泥强度等级、掺量:P42.5级普通硅酸盐水泥，水灰比1.5，设计水泥掺量20%&#xD;&#xA;5.含三轴搅拌桩导向沟,定位、泥浆处理及外运等费用&#xD;&#xA;6、清单工程量按垂直防渗墙的每组垂直长度计量。" Zcf="0" Zgj="0" Zgr="0" Zhdj="0" Zhhj="0"/>
</QdBt>
</Qdxm>
<Csxm>
<ZjCs>
<ZjCsMx Bm="041109001001" Fl="100" Je="0" Js="0" Jsjc="" Mc="安全文明施工" Xh="1" Xmlb="1">
<AqwmfMx Fl="1.5" Je="0" Js="0" Jsjc="" Mc="基本费" Xmlb="1.1"/>
<AqwmfMx Fl="0" Je="0" Js="0" Jsjc="" Mc="增加费" Xmlb="1.2"/>
<AqwmfMx Fl="0.2" Je="0" Js="0" Jsjc="" Mc="扬尘污染防治增加费" Xmlb="1.3"/>
</ZjCsMx>
<ZjCsMx Bm="041109002001" Fl="0" Je="0" Js="0" Jsjc="" Mc="夜间施工" Xh="2" Xmlb="0"/>
<ZjCsMx Bm="041109004001" Fl="0" Je="0" Js="0" Jsjc="" Mc="冬雨季施工" Xh="3" Xmlb="0"/>
<ZjCsMx Bm="041109005001" Fl="0" Je="0" Js="0" Jsjc="" Mc="行车、行人干扰" Xh="4" Xmlb="0"/>
<ZjCsMx Bm="041109006001" Fl="0" Je="0" Js="0" Jsjc="" Mc="地上、地下设施、建筑物的临时保护设施" Xh="5" Xmlb="0"/>
<ZjCsMx Bm="041109007001" Fl="0" Je="0" Js="0" Jsjc="" Mc="已完成工程及设备保护" Xh="6" Xmlb="0"/>
<ZjCsMx Bm="041109008001" Fl="0" Je="0" Js="0" Jsjc="" Mc="临时设施" Xh="7" Xmlb="0"/>
<ZjCsMx Bm="041109009001" Fl="0" Je="0" Js="0" Jsjc="" Mc="赶工措施" Xh="8" Xmlb="0"/>
<ZjCsMx Bm="041109010001" Fl="0" Je="0" Js="0" Jsjc="" Mc="工程按质论价" Xh="9" Xmlb="2"/>
<ZjCsMx Bm="041109011001" Fl="0" Je="0" Js="0" Jsjc="" Mc="建筑工人实名制费用" Xh="10" Xmlb="0"/>
</ZjCs>
<DjCs>
<DjCsMx Bm="041106001001" Clf="0" Dw="项" Fcf="0" Glf="0" Jsgz="按使用机械设备的数量计算" Jxf="0" Lr="0" Mc="大型机械设备进出场及安拆" Rgf="0" Sbf="0" Sl="1" Xh="1" Xmtz="1.机械设备名称:挖机、打桩机等满足施工要求的机械设备" Zcf="0" Zgj="0" Zgr="0" Zhdj="0" Zhhj="0"/>
</DjCs>
</Csxm>
<Qtxm>
<QtxmMx Bz="明细详见表-12-1" Je="0" Mc="暂列金额" Xh="1" Xmlb="1"/>
<QtxmMx Bz="" Je="0" Mc="暂估价" Xh="2" Xmlb="2"/>
<QtxmMx Bz="明细详见表-12-2" Je="0" Mc="材料(工程设备)暂估价" Xh="2.1" Xmlb="2.1"/>
<QtxmMx Bz="明细详见表-12-3" Je="0" Mc="专业工程暂估价" Xh="2.2" Xmlb="2.2"/>
<QtxmMx Bz="明细详见表-12-4" Je="0" Mc="计日工" Xh="3" Xmlb="3"/>
<QtxmMx Bz="明细详见表-12-5" Je="0" Mc="总承包服务费" Xh="4" Xmlb="4"/>
</Qtxm>
<Zlje/>
<Clzg/>
<Zygczg/>
<Jrg>
<JrgBt Je="0" Lb="1" Mc="人工" Xh="1"/>
<JrgBt Je="0" Lb="2" Mc="材料" Xh="2"/>
<JrgBt Je="0" Lb="3" Mc="施工机械" Xh="3"/>
<JrgBt Je="0" Lb="4" Mc="企业管理费和利润" Xh="4"/>
</Jrg>
<Zcbfwf/>
<Zjxmjdkzffj/>
<Fbrgycl/>
<Cbrgycl/>
<Rcjhz/>
</Dwgcxx>
<Dwgcxx DogNum="161618808278" Dwgcbh="002" Dwgcmc="道路工程" MachineKey="C0:3F:D5:75:B3:09" SoftName="南京未来高新技术有限公司" SoftNum="空" Zylb="4">
<Fywj/>
<Gfsj>
<GfsjMx Fl="100" Fyxlb="1" Je="0" Jsjc="分部分项工程费+措施项目费+其他项目费-除税工程设备费" Mc="规费" Qfjs="0" Xh="1"/>
<GfsjMx Fl="2" Fyxlb="1.1" Je="0" Jsjc="分部分项工程费+措施项目费+其他项目费-除税工程设备费" Mc="社会保险费" Qfjs="0" Xh="1.1"/>
<GfsjMx Fl="0.34" Fyxlb="1.2" Je="0" Jsjc="分部分项工程费+措施项目费+其他项目费-除税工程设备费" Mc="住房公积金" Qfjs="0" Xh="1.2"/>
<GfsjMx Fl="9" Fyxlb="2" Je="0" Jsjc="分部分项工程费+措施项目费+其他项目费+规费-(甲供材料费+甲供设备费)" Mc="税金" Qfjs="0" Xh="2"/>
<GfsjMx Fl="100" Fyxlb="3" Je="0" Jsjc="" Mc="合计" Qfjs="0" Xh="3"/>
</Gfsj>
<Qdxm>
<QdBt Bz="" Je="0" Mc="D.2道路工程" Xh="1" Zgj="0">
<Qdmx Bz="" Clf="0" Dw="m2" Fcf="0" Glf="0" Jsgz="按设计图示尺寸以面积计算，不扣除各类井所占面积" Jxf="0" Lr="0" Mc="砂砾石" Qdbm="040202009001" Rgf="0" Sbf="0" Sl="1340.7" Xh="1" Xmtz="1.石料规格:砂砾石垫层&#xD;&#xA;2.厚度:15cm" Zcf="0" Zgj="0" Zgr="0" Zhdj="0" Zhhj="0"/>
<Qdmx Bz="" Clf="0" Dw="m2" Fcf="0" Glf="0" Jsgz="按设计图示尺寸以面积计算，不扣除各类井所占面积" Jxf="0" Lr="0" Mc="水泥稳定碎（砾）石" Qdbm="040202015001" Rgf="0" Sbf="0" Sl="1177.2" Xh="2" Xmtz="1.水泥含量:5%水泥稳定碎石&#xD;&#xA;2.石料规格:满足设计及规范要求&#xD;&#xA;3.厚度:30cm" Zcf="0" Zgj="0" Zgr="0" Zhdj="0" Zhhj="0"/>
<Qdmx Bz="" Clf="0" Dw="m2" Fcf="0" Glf="0" Jsgz="按设计图示尺寸以面积计算，不扣除各种井所占面积，带平石的面层应扣除平石所占面积" Jxf="0" Lr="0" Mc="水泥混凝土" Qdbm="040203007001" Rgf="0" Sbf="0" Sl="981" Xh="3" Xmtz="1.混凝土强度等级:C30商品砼&#xD;&#xA;2.厚度:22cm&#xD;&#xA;3.嵌缝材料:满足设计及规范要求&#xD;&#xA;4.:含模板、切缝、灌缝、养护、扫毛等全部费用" Zcf="0" Zgj="0" Zgr="0" Zhdj="0" Zhhj="0"/>
<Qdmx Bz="" Clf="0" Dw="m" Fcf="0" Glf="0" Jsgz="按设计图示中心线长度计算" Jxf="0" Lr="0" Mc="现浇缘石" Qdbm="040204005001" Rgf="0" Sbf="0" Sl="654" Xh="4" Xmtz="1.材料品种:C25砼縁石&#xD;&#xA;2.尺寸:150*150mm&#xD;&#xA;3.基础、垫层：材料品种、厚度:C15砼垫层" Zcf="0" Zgj="0" Zgr="0" Zhdj="0" Zhhj="0"/>
<Qdmx Bz="" Clf="0" Dw="m2" Fcf="0" Glf="0" Jsgz="按设计图示尺寸以面积计算" Jxf="0" Lr="0" Mc="土工合成材料" Qdbm="040201021001" Rgf="0" Sbf="0" Sl="36160" Xh="5" Xmtz="1.材料品种、规格:加筋土工布（高韧聚酯）&#xD;&#xA;2.搭接方式:搭接&#xD;&#xA;3.:加筋土工布参数详见设计图纸&#xD;&#xA;4.:提供检测报告" Zcf="0" Zgj="0" Zgr="0" Zhdj="0" Zhhj="0"/>
<Qdmx Bz="" Clf="0" Dw="m3" Fcf="0" Glf="0" Jsgz="按设计图示尺寸以体积计算" Jxf="0" Lr="0" Mc="浆砌块料" Qdbm="040305003001" Rgf="0" Sbf="0" Sl="450" Xh="6" Xmtz="1.部位:圩堤坡脚处&#xD;&#xA;2.材料品种、规格:30cmM10浆砌片石护坡" Zcf="0" Zgj="0" Zgr="0" Zhdj="0" Zhhj="0"/>
<Qdmx Bz="" Clf="0" Dw="m2" Fcf="0" Glf="0" Jsgz="按设计图示尺寸以面积计算" Jxf="0" Lr="0" Mc="护坡" Qdbm="040305005001" Rgf="0" Sbf="0" Sl="2850" Xh="7" Xmtz="1.材料品种:人字形浆砌片石节水骨架内铺草皮护坡&#xD;&#xA;2.:参见图集93J007-8-P11" Zcf="0" Zgj="0" Zgr="0" Zhdj="0" Zhhj="0"/>
<Qdmx Bz="" Clf="0" Dw="t" Fcf="0" Glf="0" Jsgz="按设计图示尺寸以质量计算" Jxf="0" Lr="0" Mc="现浇构件钢筋" Qdbm="040901001001" Rgf="0" Sbf="0" Sl="0.124" Xh="8" Xmtz="1.钢筋种类:HRB400钢筋&#xD;&#xA;2.钢筋规格:14&#xD;&#xA;3.:拉杆钢筋" Zcf="0" Zgj="0" Zgr="0" Zhdj="0" Zhhj="0"/>
</QdBt>
</Qdxm>
<Csxm>
<ZjCs>
<ZjCsMx Bm="041109001001" Fl="100" Je="0" Js="0" Jsjc="" Mc="安全文明施工" Xh="1" Xmlb="1">
<AqwmfMx Fl="1.5" Je="0" Js="0" Jsjc="" Mc="基本费" Xmlb="1.1"/>
<AqwmfMx Fl="0" Je="0" Js="0" Jsjc="" Mc="增加费" Xmlb="1.2"/>
<AqwmfMx Fl="0.31" Je="0" Js="0" Jsjc="" Mc="扬尘污染防治增加费" Xmlb="1.3"/>
</ZjCsMx>
<ZjCsMx Bm="041109002001" Fl="0" Je="0" Js="0" Jsjc="" Mc="夜间施工" Xh="2" Xmlb="0"/>
<ZjCsMx Bm="041109004001" Fl="0" Je="0" Js="0" Jsjc="" Mc="冬雨季施工" Xh="3" Xmlb="0"/>
<ZjCsMx Bm="041109005001" Fl="0" Je="0" Js="0" Jsjc="" Mc="行车、行人干扰" Xh="4" Xmlb="0"/>
<ZjCsMx Bm="041109006001" Fl="0" Je="0" Js="0" Jsjc="" Mc="地上、地下设施、建筑物的临时保护设施" Xh="5" Xmlb="0"/>
<ZjCsMx Bm="041109007001" Fl="0" Je="0" Js="0" Jsjc="" Mc="已完成工程及设备保护" Xh="6" Xmlb="0"/>
<ZjCsMx Bm="041109008001" Fl="0" Je="0" Js="0" Jsjc="" Mc="临时设施" Xh="7" Xmlb="0"/>
<ZjCsMx Bm="041109009001" Fl="0" Je="0" Js="0" Jsjc="" Mc="赶工措施" Xh="8" Xmlb="0"/>
<ZjCsMx Bm="041109010001" Fl="0" Je="0" Js="0" Jsjc="" Mc="工程按质论价" Xh="9" Xmlb="2"/>
<ZjCsMx Bm="041109011001" Fl="0" Je="0" Js="0" Jsjc="" Mc="建筑工人实名制费用" Xh="10" Xmlb="0"/>
</ZjCs>
<DjCs/>
</Csxm>
<Qtxm>
<QtxmMx Bz="明细详见表-12-1" Je="0" Mc="暂列金额" Xh="1" Xmlb="1"/>
<QtxmMx Bz="" Je="0" Mc="暂估价" Xh="2" Xmlb="2"/>
<QtxmMx Bz="明细详见表-12-2" Je="0" Mc="材料(工程设备)暂估价" Xh="2.1" Xmlb="2.1"/>
<QtxmMx Bz="明细详见表-12-3" Je="0" Mc="专业工程暂估价" Xh="2.2" Xmlb="2.2"/>
<QtxmMx Bz="明细详见表-12-4" Je="0" Mc="计日工" Xh="3" Xmlb="3"/>
<QtxmMx Bz="明细详见表-12-5" Je="0" Mc="总承包服务费" Xh="4" Xmlb="4"/>
</Qtxm>
<Zlje/>
<Clzg/>
<Zygczg/>
<Jrg>
<JrgBt Je="0" Lb="1" Mc="人工" Xh="1"/>
<JrgBt Je="0" Lb="2" Mc="材料" Xh="2"/>
<JrgBt Je="0" Lb="3" Mc="施工机械" Xh="3"/>
<JrgBt Je="0" Lb="4" Mc="企业管理费和利润" Xh="4"/>
</Jrg>
<Zcbfwf/>
<Zjxmjdkzffj/>
<Fbrgycl/>
<Cbrgycl/>
<Rcjhz/>
</Dwgcxx>
<Dwgcxx DogNum="161618808278" Dwgcbh="003" Dwgcmc="土方工程" MachineKey="C0:3F:D5:75:B3:09" SoftName="南京未来高新技术有限公司" SoftNum="空" Zylb="4">
<Fywj/>
<Gfsj>
<GfsjMx Fl="100" Fyxlb="1" Je="0" Jsjc="分部分项工程费+措施项目费+其他项目费-除税工程设备费" Mc="规费" Qfjs="0" Xh="1"/>
<GfsjMx Fl="1.3" Fyxlb="1.1" Je="0" Jsjc="分部分项工程费+措施项目费+其他项目费-除税工程设备费" Mc="社会保险费" Qfjs="0" Xh="1.1"/>
<GfsjMx Fl="0.24" Fyxlb="1.2" Je="0" Jsjc="分部分项工程费+措施项目费+其他项目费-除税工程设备费" Mc="住房公积金" Qfjs="0" Xh="1.2"/>
<GfsjMx Fl="9" Fyxlb="2" Je="0" Jsjc="分部分项工程费+措施项目费+其他项目费+规费-(甲供材料费+甲供设备费)" Mc="税金" Qfjs="0" Xh="2"/>
<GfsjMx Fl="100" Fyxlb="3" Je="0" Jsjc="" Mc="合计" Qfjs="0" Xh="3"/>
</Gfsj>
<Qdxm>
<QdBt Bz="" Je="0" Mc="D.1土石方工程" Xh="1" Zgj="0">
<Qdmx Bz="" Clf="0" Dw="m3" Fcf="0" Glf="0" Jsgz="按设计图示尺寸以体积计算" Jxf="0" Lr="0" Mc="挖一般土方（原地面清表）" Qdbm="040101001003" Rgf="0" Sbf="0" Sl="3974.4" Xh="1" Xmtz="1.土壤类别:见设计图纸&#xD;&#xA;2.挖土深度:300mm以内&#xD;&#xA;3.:土方堆放至指定堆土区域" Zcf="0" Zgj="0" Zgr="0" Zhdj="0" Zhhj="0"/>
<Qdmx Bz="" Clf="0" Dw="m3" Fcf="0" Glf="0" Jsgz="按挖方清单项目工程量减利用回填方体积(正数)计算" Jxf="0" Lr="0" Mc="余方弃置" Qdbm="040103002002" Rgf="0" Sbf="0" Sl="3974.4" Xh="2" Xmtz="1.多余及不可利用土方弃置&#xD;&#xA;2.运距及堆场自行考虑" Zcf="0" Zgj="0" Zgr="0" Zhdj="0" Zhhj="0"/>
<Qdmx Bz="" Clf="0" Dw="m3" Fcf="0" Glf="0" Jsgz="按设计图示尺寸以体积计算" Jxf="0" Lr="0" Mc="挖一般土方" Qdbm="040101001002" Rgf="0" Sbf="0" Sl="18625.39" Xh="3" Xmtz="1.土壤类别:三类土为主，详见图纸&#xD;&#xA;2.挖土深度:4m以内&#xD;&#xA;3.:填埋库区土方开挖，边坡1:2.6，修坡、库区基底以上20cm采用人工开挖，开挖土方场内调运" Zcf="0" Zgj="0" Zgr="0" Zhdj="0" Zhhj="0"/>
<Qdmx Bz="" Clf="0" Dw="m" Fcf="0" Glf="0" Jsgz="按设计图示以长度计算" Jxf="0" Lr="0" Mc="排水沟" Qdbm="040201022001" Rgf="0" Sbf="0" Sl="360" Xh="4" Xmtz="1.断面尺寸:按设计图纸&#xD;&#xA;2.排水沟土方开挖，修整边坡" Zcf="0" Zgj="0" Zgr="0" Zhdj="0" Zhhj="0"/>
<Qdmx Bz="" Clf="0" Dw="m3" Fcf="0" Glf="0" Jsgz="按设计图示尺寸以面积计算" Jxf="0" Lr="0" Mc="袋装土保护层" Qdbm="040701007002" Rgf="0" Sbf="0" Sl="900" Xh="5" Xmtz="1.编制袋装土" Zcf="0" Zgj="0" Zgr="0" Zhdj="0" Zhhj="0"/>
<Qdmx Bz="" Clf="0" Dw="m3" Fcf="0" Glf="0" Jsgz="1.按挖方清单项目工程量加原地面线至设计要求标高间的体积，减基础、构筑物等埋入体积计算&#xA;2.按设计图示尺寸以体积计算" Jxf="0" Lr="0" Mc="8%灰土回填方" Qdbm="040103001003" Rgf="0" Sbf="0" Sl="10000" Xh="6" Xmtz="1.密实度要求:压实度满足设计及规范要求&#xD;&#xA;2.填方材料品种:8%灰土回填&#xD;&#xA;3.填方来源、运距:自行考虑" Zcf="0" Zgj="0" Zgr="0" Zhdj="0" Zhhj="0"/>
<Qdmx Bz="" Clf="0" Dw="m3" Fcf="0" Glf="0" Jsgz="1.按挖方清单项目工程量加原地面线至设计要求标高间的体积，减基础、构筑物等埋入体积计算&#xA;2.按设计图示尺寸以体积计算" Jxf="0" Lr="0" Mc="回填方（路基）" Qdbm="040103001001" Rgf="0" Sbf="0" Sl="19084.8" Xh="7" Xmtz="1.路基填土压实&#xD;&#xA;2.密实度要求 满足设计要求&#xD;&#xA;3.填方材料品种 素土&#xD;&#xA;4.填方来源、运距 自行考虑" Zcf="0" Zgj="0" Zgr="0" Zhdj="0" Zhhj="0"/>
<Qdmx Bz="" Clf="0" Dw="m3" Fcf="0" Glf="0" Jsgz="1.按挖方清单项目工程量加原地面线至设计要求标高间的体积，减基础、构筑物等埋入体积计算&#xA;2.按设计图示尺寸以体积计算" Jxf="0" Lr="0" Mc="回填方（桩基平台）" Qdbm="040103001002" Rgf="0" Sbf="0" Sl="2815.2" Xh="8" Xmtz="1.密实度要求:满足设计及规范要求&#xD;&#xA;2.填方材料品种:桩基施工平台素土回填压实&#xD;&#xA;3.填方粒径要求:满足设计及规范要求" Zcf="0" Zgj="0" Zgr="0" Zhdj="0" Zhhj="0"/>
<Qdmx Bz="" Clf="0" Dw="m3" Fcf="0" Glf="0" Jsgz="按挖方清单项目工程量减利用回填方体积(正数)计算" Jxf="0" Lr="0" Mc="缺方内进" Qdbm="040103002001" Rgf="0" Sbf="0" Sl="20517.79" Xh="9" Xmtz="1.内进回填土方，土质满足路基回填土设计及规范要求&#xD;&#xA;2.运距及购土费用自行考虑" Zcf="0" Zgj="0" Zgr="0" Zhdj="0" Zhhj="0"/>
</QdBt>
<QdBt Bz="" Je="0" Mc="D.1基底土石方工程" Xh="2" Zgj="0">
<Qdmx Bz="" Clf="0" Dw="m3" Fcf="0" Glf="0" Jsgz="按设计图示尺寸以基础垫层底面积乘以挖土深度计算" Jxf="0" Lr="0" Mc="挖沟槽土方" Qdbm="040101002002" Rgf="0" Sbf="0" Sl="91.66" Xh="10" Xmtz="1.土壤类别:三类土为主&#xD;&#xA;2.挖土深度:50cm&#xD;&#xA;3.:基底集水沟、盲沟开挖" Zcf="0" Zgj="0" Zgr="0" Zhdj="0" Zhhj="0"/>
<Qdmx Bz="" Clf="0" Dw="m2" Fcf="0" Glf="0" Jsgz="按设计道路底基层图示尺寸以面积计算，不扣除各类井所占面积" Jxf="0" Lr="0" Mc="基层、边坡修正碾压" Qdbm="040202001002" Rgf="0" Sbf="0" Sl="14342" Xh="11" Xmtz="1.部位:池底及边坡整平压实" Zcf="0" Zgj="0" Zgr="0" Zhdj="0" Zhhj="0"/>
<Qdmx Bz="" Clf="0" Dw="m3" Fcf="0" Glf="0" Jsgz="按设计图示尺寸以面积计算" Jxf="0" Lr="0" Mc="压实黏土防渗层" Qdbm="040701003001" Rgf="0" Sbf="0" Sl="2221" Xh="12" Xmtz="1.厚度:500mm压实黏土&#xD;&#xA;2.渗透系数:≤10-5cm/s&#xD;&#xA;3.:含土方开挖、运输、回填、碾压" Zcf="0" Zgj="0" Zgr="0" Zhdj="0" Zhhj="0"/>
</QdBt>
<QdBt Bz="" Je="0" Mc="D.1锚固沟土石方工程" Xh="3" Zgj="0">
<Qdmx Bz="" Clf="0" Dw="m3" Fcf="0" Glf="0" Jsgz="按设计图示尺寸以基础垫层底面积乘以挖土深度计算" Jxf="0" Lr="0" Mc="挖沟槽土方" Qdbm="040101002003" Rgf="0" Sbf="0" Sl="396" Xh="13" Xmtz="1.土壤类别:三类土为主&#xD;&#xA;2.挖土深度:120cm&#xD;&#xA;3.:锚固沟" Zcf="0" Zgj="0" Zgr="0" Zhdj="0" Zhhj="0"/>
<Qdmx Bz="" Clf="0" Dw="m3" Fcf="0" Glf="0" Jsgz="1.按挖方清单项目工程量加原地面线至设计要求标高间的体积，减基础、构筑物等埋入体积计算&#xA;2.按设计图示尺寸以体积计算" Jxf="0" Lr="0" Mc="回填方" Qdbm="040103001004" Rgf="0" Sbf="0" Sl="132" Xh="14" Xmtz="1.密实度要求:满足设计及规范要求&#xD;&#xA;2.填方材料品种:素土&#xD;&#xA;3.填方来源、运距:利用开挖土方" Zcf="0" Zgj="0" Zgr="0" Zhdj="0" Zhhj="0"/>
</QdBt>
<QdBt Bz="" Je="0" Mc="D.1水池土方工程" Xh="4" Zgj="0">
<Qdmx Bz="" Clf="0" Dw="m3" Fcf="0" Glf="0" Jsgz="按设计图示尺寸以体积计算" Jxf="0" Lr="0" Mc="挖一般土方" Qdbm="040101001004" Rgf="0" Sbf="0" Sl="2259.98" Xh="15" Xmtz="1.土壤类别:三类土为主&#xD;&#xA;2.挖土深度:详见设计图纸" Zcf="0" Zgj="0" Zgr="0" Zhdj="0" Zhhj="0"/>
<Qdmx Bz="" Clf="0" Dw="m3" Fcf="0" Glf="0" Jsgz="1.按挖方清单项目工程量加原地面线至设计要求标高间的体积，减基础、构筑物等埋入体积计算&#xA;2.按设计图示尺寸以体积计算" Jxf="0" Lr="0" Mc="回填方" Qdbm="040103001005" Rgf="0" Sbf="0" Sl="1288.6" Xh="16" Xmtz="1.密实度要求:满足设计及规范要求&#xD;&#xA;2.填方材料品种:素土&#xD;&#xA;3.填方来源、运距:自行考虑" Zcf="0" Zgj="0" Zgr="0" Zhdj="0" Zhhj="0"/>
</QdBt>
<QdBt Bz="" Je="0" Mc="D.1排水沟土石方工程" Xh="5" Zgj="0">
<Qdmx Bz="" Clf="0" Dw="m3" Fcf="0" Glf="0" Jsgz="按设计图示尺寸以基础垫层底面积乘以挖土深度计算" Jxf="0" Lr="0" Mc="挖沟槽土方" Qdbm="040101002004" Rgf="0" Sbf="0" Sl="756" Xh="17" Xmtz="1.土壤类别:三类土为主&#xD;&#xA;2.挖土深度:120cm&#xD;&#xA;3.:锚固沟" Zcf="0" Zgj="0" Zgr="0" Zhdj="0" Zhhj="0"/>
<Qdmx Bz="" Clf="0" Dw="m3" Fcf="0" Glf="0" Jsgz="1.按挖方清单项目工程量加原地面线至设计要求标高间的体积，减基础、构筑物等埋入体积计算&#xA;2.按设计图示尺寸以体积计算" Jxf="0" Lr="0" Mc="回填方" Qdbm="040103001006" Rgf="0" Sbf="0" Sl="235.8" Xh="18" Xmtz="1.密实度要求:满足设计及规范要求&#xD;&#xA;2.填方材料品种:素土&#xD;&#xA;3.填方来源、运距:利用开挖土方" Zcf="0" Zgj="0" Zgr="0" Zhdj="0" Zhhj="0"/>
</QdBt>
</Qdxm>
<Csxm>
<ZjCs>
<ZjCsMx Bm="041109001001" Fl="100" Je="0" Js="0" Jsjc="" Mc="安全文明施工" Xh="1" Xmlb="1">
<AqwmfMx Fl="1.5" Je="0" Js="0" Jsjc="" Mc="基本费" Xmlb="1.1"/>
<AqwmfMx Fl="0" Je="0" Js="0" Jsjc="" Mc="增加费" Xmlb="1.2"/>
<AqwmfMx Fl="0.42" Je="0" Js="0" Jsjc="" Mc="扬尘污染防治增加费" Xmlb="1.3"/>
</ZjCsMx>
<ZjCsMx Bm="041109002001" Fl="0" Je="0" Js="0" Jsjc="" Mc="夜间施工" Xh="2" Xmlb="0"/>
<ZjCsMx Bm="041109004001" Fl="0" Je="0" Js="0" Jsjc="" Mc="冬雨季施工" Xh="3" Xmlb="0"/>
<ZjCsMx Bm="041109005001" Fl="0" Je="0" Js="0" Jsjc="" Mc="行车、行人干扰" Xh="4" Xmlb="0"/>
<ZjCsMx Bm="041109006001" Fl="0" Je="0" Js="0" Jsjc="" Mc="地上、地下设施、建筑物的临时保护设施" Xh="5" Xmlb="0"/>
<ZjCsMx Bm="041109007001" Fl="0" Je="0" Js="0" Jsjc="" Mc="已完成工程及设备保护" Xh="6" Xmlb="0"/>
<ZjCsMx Bm="041109008001" Fl="0" Je="0" Js="0" Jsjc="" Mc="临时设施" Xh="7" Xmlb="0"/>
<ZjCsMx Bm="041109009001" Fl="0" Je="0" Js="0" Jsjc="" Mc="赶工措施" Xh="8" Xmlb="0"/>
<ZjCsMx Bm="041109010001" Fl="0" Je="0" Js="0" Jsjc="" Mc="工程按质论价" Xh="9" Xmlb="2"/>
<ZjCsMx Bm="041109011001" Fl="0" Je="0" Js="0" Jsjc="" Mc="建筑工人实名制费用" Xh="10" Xmlb="0"/>
</ZjCs>
<DjCs>
<DjCsMx Bm="041106001001" Clf="0" Dw="项" Fcf="0" Glf="0" Jsgz="按使用机械设备的数量计算" Jxf="0" Lr="0" Mc="大型机械设备进出场及安拆" Rgf="0" Sbf="0" Sl="1" Xh="1" Xmtz="1.机械设备名称:满足施工要求的大型机械设备" Zcf="0" Zgj="0" Zgr="0" Zhdj="0" Zhhj="0"/>
<DjCsMx Bm="041107002001" Clf="0" Dw="项" Fcf="0" Glf="0" Jsgz="按排、降水日历天数计算" Jxf="0" Lr="0" Mc="排水、降水" Rgf="0" Sbf="0" Sl="1" Xh="2" Xmtz="1.基坑排水、降水，考虑机械设备使用费用，使用井和使用天数按实计量" Zcf="0" Zgj="0" Zgr="0" Zhdj="0" Zhhj="0"/>
</DjCs>
</Csxm>
<Qtxm>
<QtxmMx Bz="明细详见表-12-1" Je="0" Mc="暂列金额" Xh="1" Xmlb="1"/>
<QtxmMx Bz="" Je="0" Mc="暂估价" Xh="2" Xmlb="2"/>
<QtxmMx Bz="明细详见表-12-2" Je="0" Mc="材料(工程设备)暂估价" Xh="2.1" Xmlb="2.1"/>
<QtxmMx Bz="明细详见表-12-3" Je="0" Mc="专业工程暂估价" Xh="2.2" Xmlb="2.2"/>
<QtxmMx Bz="明细详见表-12-4" Je="0" Mc="计日工" Xh="3" Xmlb="3"/>
<QtxmMx Bz="明细详见表-12-5" Je="0" Mc="总承包服务费" Xh="4" Xmlb="4"/>
</Qtxm>
<Zlje/>
<Clzg/>
<Zygczg/>
<Jrg>
<JrgBt Je="0" Lb="1" Mc="人工" Xh="1"/>
<JrgBt Je="0" Lb="2" Mc="材料" Xh="2"/>
<JrgBt Je="0" Lb="3" Mc="施工机械" Xh="3"/>
<JrgBt Je="0" Lb="4" Mc="企业管理费和利润" Xh="4"/>
</Jrg>
<Zcbfwf/>
<Zjxmjdkzffj/>
<Fbrgycl/>
<Cbrgycl/>
<Rcjhz/>
</Dwgcxx>
<Dwgcxx DogNum="161618808278" Dwgcbh="004" Dwgcmc="防渗工程" MachineKey="C0:3F:D5:75:B3:09" SoftName="南京未来高新技术有限公司" SoftNum="空" Zylb="4">
<Fywj/>
<Gfsj>
<GfsjMx Fl="100" Fyxlb="1" Je="0" Jsjc="分部分项工程费+措施项目费+其他项目费-除税工程设备费" Mc="规费" Qfjs="0" Xh="1"/>
<GfsjMx Fl="2" Fyxlb="1.1" Je="0" Jsjc="分部分项工程费+措施项目费+其他项目费-除税工程设备费" Mc="社会保险费" Qfjs="0" Xh="1.1"/>
<GfsjMx Fl="0.34" Fyxlb="1.2" Je="0" Jsjc="分部分项工程费+措施项目费+其他项目费-除税工程设备费" Mc="住房公积金" Qfjs="0" Xh="1.2"/>
<GfsjMx Fl="9" Fyxlb="2" Je="0" Jsjc="分部分项工程费+措施项目费+其他项目费+规费-(甲供材料费+甲供设备费)" Mc="税金" Qfjs="0" Xh="2"/>
<GfsjMx Fl="100" Fyxlb="3" Je="0" Jsjc="" Mc="合计" Qfjs="0" Xh="3"/>
</Gfsj>
<Qdxm>
<QdBt Bz="" Je="0" Mc="D.7填埋库区底面防渗工程" Xh="1" Zgj="0">
<Qdmx Bz="" Clf="0" Dw="m2" Fcf="0" Glf="0" Jsgz="按设计图示尺寸以面积计算" Jxf="0" Lr="0" Mc="双光面HDPE土工膜（1.5mm厚）" Qdbm="040701004007" Rgf="0" Sbf="0" Sl="4442" Xh="1" Xmtz="1.铺设位置:池底次防渗层&#xD;&#xA;2.材料规格、强度、单位重量:双光面HDPE土工膜（1.5mm厚）（进口膜）&#xD;&#xA;3.连（搭）接方式:焊接&#xD;&#xA;4.:技术要求详见设计图纸" Zcf="0" Zgj="0" Zgr="0" Zhdj="0" Zhhj="0"/>
<Qdmx Bz="" Clf="0" Dw="m2" Fcf="0" Glf="0" Jsgz="按设计图示尺寸以面积计算" Jxf="0" Lr="0" Mc="双光面HDPE土工膜（2.0mm厚）" Qdbm="040701004008" Rgf="0" Sbf="0" Sl="4442" Xh="2" Xmtz="1.铺设位置:池底主防渗层&#xD;&#xA;2.材料规格、强度、单位重量:双光面HDPE土工膜（2.0mm厚）（进口膜）&#xD;&#xA;3.连（搭）接方式:焊接&#xD;&#xA;4.:技术要求详见设计图纸" Zcf="0" Zgj="0" Zgr="0" Zhdj="0" Zhhj="0"/>
<Qdmx Bz="" Clf="0" Dw="m2" Fcf="0" Glf="0" Jsgz="按设计图示尺寸以面积计算" Jxf="0" Lr="0" Mc="土工排水网格" Qdbm="040701006004" Rgf="0" Sbf="0" Sl="5442" Xh="3" Xmtz="1.铺设位置:池底渗漏检测层&#xD;&#xA;2.厚度、防渗系数:7.5mm&#xD;&#xA;3.材料规格、强度、单位重量:三维复合土工排水网格，HDPE材质，详见设计图纸&#xD;&#xA;4.连（搭）接方式:搭接" Zcf="0" Zgj="0" Zgr="0" Zhdj="0" Zhhj="0"/>
<Qdmx Bz="" Clf="0" Dw="m2" Fcf="0" Glf="0" Jsgz="按设计图示尺寸以面积计算" Jxf="0" Lr="0" Mc="长丝无纺布（600g/m2)" Qdbm="040701006005" Rgf="0" Sbf="0" Sl="9053" Xh="4" Xmtz="1.铺设位置:池底防渗保护层&#xD;&#xA;2.厚度、防渗系数:600g/m2&#xD;&#xA;3.材料规格、强度、单位重量:长丝无纺土工布600g/m2&#xD;&#xA;4.连（搭）接方式:缝合" Zcf="0" Zgj="0" Zgr="0" Zhdj="0" Zhhj="0"/>
</QdBt>
<QdBt Bz="" Je="0" Mc="D.7填埋库区坡面防渗工程" Xh="2" Zgj="0">
<Qdmx Bz="" Clf="0" Dw="m2" Fcf="0" Glf="0" Jsgz="按设计图示尺寸以面积计算" Jxf="0" Lr="0" Mc="长丝土工布（600g/m2)" Qdbm="040701006007" Rgf="0" Sbf="0" Sl="17654" Xh="5" Xmtz="1.铺设位置:边坡防渗&#xD;&#xA;2.材料规格、强度、单位重量:600g/m2针刺长丝土工布，双层&#xD;&#xA;3.材料性能要求见设计图纸" Zcf="0" Zgj="0" Zgr="0" Zhdj="0" Zhhj="0"/>
<Qdmx Bz="" Clf="0" Dw="m2" Fcf="0" Glf="0" Jsgz="按设计图示尺寸以面积计算" Jxf="0" Lr="0" Mc="双毛面HDPE土工膜（1.5mm厚）" Qdbm="040701004009" Rgf="0" Sbf="0" Sl="8667" Xh="6" Xmtz="1.铺设位置:边坡次防渗层&#xD;&#xA;2.材料规格、强度、单位重量:双毛面HHDPE土工膜（1.5mm厚）（进口膜）&#xD;&#xA;3.连（搭）接方式:焊接&#xD;&#xA;4.:技术要求详见设计图纸" Zcf="0" Zgj="0" Zgr="0" Zhdj="0" Zhhj="0"/>
<Qdmx Bz="" Clf="0" Dw="m2" Fcf="0" Glf="0" Jsgz="按设计图示尺寸以面积计算" Jxf="0" Lr="0" Mc="土工排水网格" Qdbm="040701006008" Rgf="0" Sbf="0" Sl="10334" Xh="7" Xmtz="1.铺设位置:池底渗漏检测层&#xD;&#xA;2.厚度、防渗系数:6.3mm&#xD;&#xA;3.材料规格、强度、单位重量:三维复合土工排水网格，HDPE材质，详见设计图纸&#xD;&#xA;4.连（搭）接方式:搭接" Zcf="0" Zgj="0" Zgr="0" Zhdj="0" Zhhj="0"/>
<Qdmx Bz="" Clf="0" Dw="m2" Fcf="0" Glf="0" Jsgz="按设计图示尺寸以面积计算" Jxf="0" Lr="0" Mc="双毛面HDPE土工膜（2.0mm厚）" Qdbm="040701006009" Rgf="0" Sbf="0" Sl="8667" Xh="8" Xmtz="1.铺设位置:边坡主防渗层&#xD;&#xA;2.材料规格、强度、单位重量:双毛面HHDPE土工膜（2.0mm厚）（进口膜）&#xD;&#xA;3.连（搭）接方式:焊接&#xD;&#xA;4.技术要求详见设计图纸" Zcf="0" Zgj="0" Zgr="0" Zhdj="0" Zhhj="0"/>
</QdBt>
<QdBt Bz="" Je="0" Mc="D.7锚固沟工程" Xh="3" Zgj="0">
<Qdmx Bz="" Clf="0" Dw="m3" Fcf="0" Glf="0" Jsgz="按设计图示尺寸以体积计算" Jxf="0" Lr="0" Mc="混凝土垫层" Qdbm="040303001001" Rgf="0" Sbf="0" Sl="264" Xh="9" Xmtz="1.混凝土强度等级:C15素砼垫层&#xD;&#xA;2.:80*80cm" Zcf="0" Zgj="0" Zgr="0" Zhdj="0" Zhhj="0"/>
</QdBt>
<QdBt Bz="" Je="0" Mc="D.5地下水导排" Xh="4" Zgj="0">
<Qdmx Bz="" Clf="0" Dw="m" Fcf="0" Glf="0" Jsgz="按设计图示尺寸以长度计算" Jxf="0" Lr="0" Mc="HDPE穿孔实壁管（De225）" Qdbm="040701010002" Rgf="0" Sbf="0" Sl="65" Xh="10" Xmtz="1.材质及规格 HDPE穿孔管（De225mm），SDR17，PE100，地下水集水主管，包含端帽&#xD;&#xA;2.连接形式 焊接&#xD;&#xA;3.铺设深度 满足图纸及规范要求&#xD;&#xA;4. 包含附件材料在内&#xD;&#xA;" Zcf="0" Zgj="0" Zgr="0" Zhdj="0" Zhhj="0"/>
<Qdmx Bz="" Clf="0" Dw="m" Fcf="0" Glf="0" Jsgz="按设计图示尺寸以长度计算" Jxf="0" Lr="0" Mc="HDPE穿孔实壁管（De160）" Qdbm="040701011003" Rgf="0" Sbf="0" Sl="140" Xh="11" Xmtz="1.材质及规格 HDPE实壁穿孔实壁管，De160，SDR17， PE100，地下水集水支管，包含端帽&#xD;&#xA;2.连接形式 焊接&#xD;&#xA;3.铺设深度 满足图纸及规范要求&#xD;&#xA;" Zcf="0" Zgj="0" Zgr="0" Zhdj="0" Zhhj="0"/>
<Qdmx Bz="" Clf="0" Dw="m" Fcf="0" Glf="0" Jsgz="按设计图示尺寸以长度计算" Jxf="0" Lr="0" Mc="HDPE实壁管（De90）" Qdbm="040701011007" Rgf="0" Sbf="0" Sl="10" Xh="12" Xmtz="1.材质及规格 HDPE实壁管，De90，SDR21， PE100&#xD;&#xA;2.连接形式 焊接&#xD;&#xA;3.铺设深度 满足图纸及规范要求&#xD;&#xA;" Zcf="0" Zgj="0" Zgr="0" Zhdj="0" Zhhj="0"/>
<Qdmx Bz="" Clf="0" Dw="m" Fcf="0" Glf="0" Jsgz="按设计图示中心线长度以延长米计算。不扣除附属构筑物、管件及阀门等所占长度" Jxf="0" Lr="0" Mc="加强软管（De90）" Qdbm="040501004001" Rgf="0" Sbf="0" Sl="30" Xh="13" Xmtz="1.材质及规格 加强弹性软管（De90），地下水收集软管，含尼龙绳等配件&#xD;&#xA;2.铺设深度 详见图纸&#xD;&#xA;" Zcf="0" Zgj="0" Zgr="0" Zhdj="0" Zhhj="0"/>
<Qdmx Bz="" Clf="0" Dw="m" Fcf="0" Glf="0" Jsgz="按设计图示尺寸以长度计算" Jxf="0" Lr="0" Mc="HDPE实壁管铺设（De800）" Qdbm="040701011008" Rgf="0" Sbf="0" Sl="22" Xh="14" Xmtz="1.材质及规格 HDPE无孔实壁管（De800mm），SDR11，PE100&#xD;&#xA;2.连接形式 焊接，200mm宽2mmHDPE膜焊接到加强膜&#xD;&#xA;3.铺设深度 满足图纸及规范要求&#xD;&#xA;4. 包含附件材料在内&#xD;&#xA;5.管道水压试验" Zcf="0" Zgj="0" Zgr="0" Zhdj="0" Zhhj="0"/>
<Qdmx Bz="" Clf="0" Dw="m3" Fcf="0" Glf="0" Jsgz="按设计图示尺寸以体积计算" Jxf="0" Lr="0" Mc="排水沟碎石回填" Qdbm="040701009005" Rgf="0" Sbf="0" Sl="85.4" Xh="15" Xmtz="1.石料 集水沟20~60mm砾石回填，规格满足设计及规范要求&#xD;&#xA;&#xD;&#xA;&#xD;&#xA;" Zcf="0" Zgj="0" Zgr="0" Zhdj="0" Zhhj="0"/>
<Qdmx Bz="" Clf="0" Dw="m2" Fcf="0" Glf="0" Jsgz="按设计图示尺寸以面积计算" Jxf="0" Lr="0" Mc="土工滤网（200g/m2)" Qdbm="040701006011" Rgf="0" Sbf="0" Sl="4445" Xh="16" Xmtz="1.铺设位置:池底支撑反滤层&#xD;&#xA;2.厚度、防渗系数:200g/m2&#xD;&#xA;3.材料规格、强度、单位重量:聚丙烯有纺土工布200g/m2&#xD;&#xA;4.连（搭）接方式:缝合" Zcf="0" Zgj="0" Zgr="0" Zhdj="0" Zhhj="0"/>
<Qdmx Bz="" Clf="0" Dw="m2" Fcf="0" Glf="0" Jsgz="按设计图示尺寸以面积计算" Jxf="0" Lr="0" Mc="无纺土工布（400g/m2)" Qdbm="040701006012" Rgf="0" Sbf="0" Sl="4445" Xh="17" Xmtz="1.铺设位置:支撑层防渗&#xD;&#xA;2.材料规格、强度、单位重量:400g/m2针刺长丝土工布&#xD;&#xA;3.材料性能要求见设计图纸" Zcf="0" Zgj="0" Zgr="0" Zhdj="0" Zhhj="0"/>
<Qdmx Bz="" Clf="0" Dw="m3" Fcf="0" Glf="0" Jsgz="按设计图示尺寸以体积计算" Jxf="0" Lr="0" Mc="混凝土垫层" Qdbm="040303001002" Rgf="0" Sbf="0" Sl="138" Xh="18" Xmtz="1.混凝土强度等级:C20素砼垫层&#xD;&#xA;2.:80*80cm" Zcf="0" Zgj="0" Zgr="0" Zhdj="0" Zhhj="0"/>
</QdBt>
<QdBt Bz="" Je="0" Mc="D.5渗滤液导排管" Xh="5" Zgj="0">
<Qdmx Bz="" Clf="0" Dw="m" Fcf="0" Glf="0" Jsgz="按设计图示尺寸以长度计算" Jxf="0" Lr="0" Mc="HDPE穿孔实壁管（De225）" Qdbm="040701010003" Rgf="0" Sbf="0" Sl="65" Xh="19" Xmtz="1.材质及规格 HDPE穿孔管（De225mm），SDR17，PE100，渗滤液集水主管，包含端帽&#xD;&#xA;2.连接形式 焊接&#xD;&#xA;3.铺设深度 满足图纸及规范要求&#xD;&#xA;4. 包含附件材料在内&#xD;&#xA;" Zcf="0" Zgj="0" Zgr="0" Zhdj="0" Zhhj="0"/>
<Qdmx Bz="" Clf="0" Dw="m" Fcf="0" Glf="0" Jsgz="按设计图示尺寸以长度计算" Jxf="0" Lr="0" Mc="HDPE穿孔实壁管（De160）" Qdbm="040701011009" Rgf="0" Sbf="0" Sl="140" Xh="20" Xmtz="1.材质及规格 HDPE实壁穿孔实壁管，De160，SDR17， PE100，渗滤液集水管，包含端帽&#xD;&#xA;2.连接形式 焊接&#xD;&#xA;3.铺设深度 满足图纸及规范要求&#xD;&#xA;" Zcf="0" Zgj="0" Zgr="0" Zhdj="0" Zhhj="0"/>
<Qdmx Bz="" Clf="0" Dw="m" Fcf="0" Glf="0" Jsgz="按设计图示尺寸以长度计算" Jxf="0" Lr="0" Mc="HDPE实壁管（De90）" Qdbm="040701011010" Rgf="0" Sbf="0" Sl="90" Xh="21" Xmtz="1.材质及规格 HDPE实壁管，De90，SDR21， PE100，渗滤液排放管&#xD;&#xA;2.连接形式 焊接&#xD;&#xA;3.铺设深度 满足图纸及规范要求&#xD;&#xA;" Zcf="0" Zgj="0" Zgr="0" Zhdj="0" Zhhj="0"/>
<Qdmx Bz="" Clf="0" Dw="m" Fcf="0" Glf="0" Jsgz="按设计图示中心线长度以延长米计算。不扣除附属构筑物、管件及阀门等所占长度" Jxf="0" Lr="0" Mc="加强软管（De90）" Qdbm="040501004002" Rgf="0" Sbf="0" Sl="30" Xh="22" Xmtz="1.材质及规格 加强弹性软管（De90），地下水收集软管，含尼龙绳等配件&#xD;&#xA;2.铺设深度 详见图纸&#xD;&#xA;" Zcf="0" Zgj="0" Zgr="0" Zhdj="0" Zhhj="0"/>
<Qdmx Bz="" Clf="0" Dw="m" Fcf="0" Glf="0" Jsgz="按设计图示尺寸以长度计算" Jxf="0" Lr="0" Mc="HDPE实壁管铺设（De800）" Qdbm="040701011011" Rgf="0" Sbf="0" Sl="44" Xh="23" Xmtz="1.材质及规格 HDPE无孔实壁管（De800mm），SDR11，PE100,含盖板&#xD;&#xA;2.连接形式 焊接，200mm宽2mmHDPE膜焊接到加强膜&#xD;&#xA;3.铺设深度 满足图纸及规范要求&#xD;&#xA;4. 包含附件材料在内&#xD;&#xA;5.管道水压试验" Zcf="0" Zgj="0" Zgr="0" Zhdj="0" Zhhj="0"/>
<Qdmx Bz="" Clf="0" Dw="m3" Fcf="0" Glf="0" Jsgz="按设计图示尺寸以体积计算" Jxf="0" Lr="0" Mc="碎（卵）石导流层" Qdbm="040701009008" Rgf="0" Sbf="0" Sl="1234" Xh="24" Xmtz="1.石料 渗滤液导流层，规格满足设计及规范要求&#xD;&#xA;2.厚度 300mm厚&#xD;&#xA;" Zcf="0" Zgj="0" Zgr="0" Zhdj="0" Zhhj="0"/>
<Qdmx Bz="" Clf="0" Dw="m3" Fcf="0" Glf="0" Jsgz="按设计图示尺寸以体积计算" Jxf="0" Lr="0" Mc="排水沟碎石回填" Qdbm="040701009006" Rgf="0" Sbf="0" Sl="39.67" Xh="25" Xmtz="1.石料 集水沟20~60mm砾石回填，规格满足设计及规范要求&#xD;&#xA;&#xD;&#xA;&#xD;&#xA;" Zcf="0" Zgj="0" Zgr="0" Zhdj="0" Zhhj="0"/>
<Qdmx Bz="" Clf="0" Dw="m3" Fcf="0" Glf="0" Jsgz="按设计图示尺寸以体积计算" Jxf="0" Lr="0" Mc="粗砂回填" Qdbm="040701009007" Rgf="0" Sbf="0" Sl="99.98" Xh="26" Xmtz="1.导排管粗砂包裹" Zcf="0" Zgj="0" Zgr="0" Zhdj="0" Zhhj="0"/>
<Qdmx Bz="" Clf="0" Dw="m2" Fcf="0" Glf="0" Jsgz="按设计图示尺寸以面积计算" Jxf="0" Lr="0" Mc="土工滤网（200g/m2)" Qdbm="040701006013" Rgf="0" Sbf="0" Sl="1657.04" Xh="27" Xmtz="1.铺设位置:池底支撑反滤层&#xD;&#xA;2.厚度、防渗系数:200g/m2&#xD;&#xA;3.材料规格、强度、单位重量:聚丙烯有纺土工布200g/m2&#xD;&#xA;4.连（搭）接方式:缝合" Zcf="0" Zgj="0" Zgr="0" Zhdj="0" Zhhj="0"/>
<Qdmx Bz="" Clf="0" Dw="m" Fcf="0" Glf="0" Jsgz="按设计图示中心线长度以延长米计算。不扣除附属构筑物、管件及阀门等所占长度" Jxf="0" Lr="0" Mc="DN100钢管" Qdbm="040501002001" Rgf="0" Sbf="0" Sl="30" Xh="28" Xmtz="1.材质及规格:DN100钢套管&#xD;&#xA;2.接口方式:焊接" Zcf="0" Zgj="0" Zgr="0" Zhdj="0" Zhhj="0"/>
</QdBt>
<QdBt Bz="" Je="0" Mc="D.5地表水导排工程" Xh="6" Zgj="0">
<Qdmx Bz="" Clf="0" Dw="m" Fcf="0" Glf="0" Jsgz="按设计图示中心线长度以延长米计算。不扣除附属构筑物、管件及阀门等所占长度" Jxf="0" Lr="0" Mc="DN500混凝土管" Qdbm="040501001002" Rgf="0" Sbf="0" Sl="50" Xh="29" Xmtz="1.垫层、基础材质及厚度:10cmC15素砼垫层 &#xD;&#xA;2.管座材质:135°C30砼管道基础及管座（含钢筋）&#xD;&#xA;3.规格:DN500Ⅱ级钢筋砼管&#xD;&#xA;4.接口方式:橡胶圈密封承插连接&#xD;&#xA;5.铺设深度:见设计图纸&#xD;&#xA;6.管道检验及试验要求:管道闭水试验" Zcf="0" Zgj="0" Zgr="0" Zhdj="0" Zhhj="0"/>
<Qdmx Bz="" Clf="0" Dw="m" Fcf="0" Glf="0" Jsgz="按设计图示尺寸以延长米计算" Jxf="0" Lr="0" Mc="混凝土渠道" Qdbm="040501019001" Rgf="0" Sbf="0" Sl="420" Xh="30" Xmtz="1.断面规格:宽600mm，深度300~600mm&#xD;&#xA;2.垫层、基础材质及厚度:C15素砼垫层&#xD;&#xA;3.混凝土强度等级:C20砼基础及井壁" Zcf="0" Zgj="0" Zgr="0" Zhdj="0" Zhhj="0"/>
<Qdmx Bz="" Clf="0" Dw="m" Fcf="0" Glf="0" Jsgz="按设计图示尺寸以延长米计算" Jxf="0" Lr="0" Mc="明沟盖板" Qdbm="040501019002" Rgf="0" Sbf="0" Sl="22" Xh="31" Xmtz="1.断面规格:宽度900&#xD;&#xA;2.预制钢筋砼明沟盖板" Zcf="0" Zgj="0" Zgr="0" Zhdj="0" Zhhj="0"/>
<Qdmx Bz="" Clf="0" Dw="座" Fcf="0" Glf="0" Jsgz="按设计图示数量计算" Jxf="0" Lr="0" Mc="混凝土出水口" Qdbm="040504007001" Rgf="0" Sbf="0" Sl="1" Xh="32" Xmtz="1.参见图集《排水管道出水口》（95S517）&#xD;&#xA;2.DN500出水口，钢筋砼" Zcf="0" Zgj="0" Zgr="0" Zhdj="0" Zhhj="0"/>
<Qdmx Bz="" Clf="0" Dw="t" Fcf="0" Glf="0" Jsgz="按设计图示尺寸以质量计算" Jxf="0" Lr="0" Mc="现浇构件钢筋" Qdbm="040901001001" Rgf="0" Sbf="0" Sl="17.056" Xh="33" Xmtz="1.钢筋种类:HPB300&#xD;&#xA;2.钢筋规格:10以内" Zcf="0" Zgj="0" Zgr="0" Zhdj="0" Zhhj="0"/>
</QdBt>
<QdBt Bz="" Je="0" Mc="D.7生活垃圾处理工程" Xh="7" Zgj="0">
<Qdmx Bz="" Clf="0" Dw="口" Fcf="0" Glf="0" Jsgz="按设计图示数量计算" Jxf="0" Lr="0" Mc="监测井" Qdbm="040701016001" Rgf="0" Sbf="0" Sl="5" Xh="34" Xmtz="1.钻孔孔径、深度:50m&#xD;&#xA;2.监测井材料、直径、壁厚、连接方式:D160HDPE实壁管&#xD;&#xA;3.滤料材质:碎石&#xD;&#xA;4.详见设计图纸" Zcf="0" Zgj="0" Zgr="0" Zhdj="0" Zhhj="0"/>
</QdBt>
</Qdxm>
<Csxm>
<ZjCs>
<ZjCsMx Bm="041109001001" Fl="100" Je="0" Js="0" Jsjc="" Mc="安全文明施工" Xh="1" Xmlb="1">
<AqwmfMx Fl="1.5" Je="0" Js="0" Jsjc="" Mc="基本费" Xmlb="1.1"/>
<AqwmfMx Fl="0" Je="0" Js="0" Jsjc="" Mc="增加费" Xmlb="1.2"/>
<AqwmfMx Fl="0.31" Je="0" Js="0" Jsjc="" Mc="扬尘污染防治增加费" Xmlb="1.3"/>
</ZjCsMx>
<ZjCsMx Bm="041109002001" Fl="0" Je="0" Js="0" Jsjc="" Mc="夜间施工" Xh="2" Xmlb="0"/>
<ZjCsMx Bm="041109004001" Fl="0" Je="0" Js="0" Jsjc="" Mc="冬雨季施工" Xh="3" Xmlb="0"/>
<ZjCsMx Bm="041109005001" Fl="0" Je="0" Js="0" Jsjc="" Mc="行车、行人干扰" Xh="4" Xmlb="0"/>
<ZjCsMx Bm="041109006001" Fl="0" Je="0" Js="0" Jsjc="" Mc="地上、地下设施、建筑物的临时保护设施" Xh="5" Xmlb="0"/>
<ZjCsMx Bm="041109007001" Fl="0" Je="0" Js="0" Jsjc="" Mc="已完成工程及设备保护" Xh="6" Xmlb="0"/>
<ZjCsMx Bm="041109008001" Fl="0" Je="0" Js="0" Jsjc="" Mc="临时设施" Xh="7" Xmlb="0"/>
<ZjCsMx Bm="041109009001" Fl="0" Je="0" Js="0" Jsjc="" Mc="赶工措施" Xh="8" Xmlb="0"/>
<ZjCsMx Bm="041109010001" Fl="0" Je="0" Js="0" Jsjc="" Mc="工程按质论价" Xh="9" Xmlb="2"/>
<ZjCsMx Bm="041109011001" Fl="0" Je="0" Js="0" Jsjc="" Mc="建筑工人实名制费用" Xh="10" Xmlb="0"/>
</ZjCs>
<DjCs/>
</Csxm>
<Qtxm>
<QtxmMx Bz="明细详见表-12-1" Je="0" Mc="暂列金额" Xh="1" Xmlb="1"/>
<QtxmMx Bz="" Je="0" Mc="暂估价" Xh="2" Xmlb="2"/>
<QtxmMx Bz="明细详见表-12-2" Je="0" Mc="材料(工程设备)暂估价" Xh="2.1" Xmlb="2.1"/>
<QtxmMx Bz="明细详见表-12-3" Je="0" Mc="专业工程暂估价" Xh="2.2" Xmlb="2.2"/>
<QtxmMx Bz="明细详见表-12-4" Je="0" Mc="计日工" Xh="3" Xmlb="3"/>
<QtxmMx Bz="明细详见表-12-5" Je="0" Mc="总承包服务费" Xh="4" Xmlb="4"/>
</Qtxm>
<Zlje/>
<Clzg/>
<Zygczg/>
<Jrg>
<JrgBt Je="0" Lb="1" Mc="人工" Xh="1"/>
<JrgBt Je="0" Lb="2" Mc="材料" Xh="2"/>
<JrgBt Je="0" Lb="3" Mc="施工机械" Xh="3"/>
<JrgBt Je="0" Lb="4" Mc="企业管理费和利润" Xh="4"/>
</Jrg>
<Zcbfwf/>
<Zjxmjdkzffj/>
<Fbrgycl/>
<Cbrgycl/>
<Rcjhz/>
</Dwgcxx>
<Dwgcxx DogNum="161618808278" Dwgcbh="005" Dwgcmc="张家港应急飞灰库安装" MachineKey="C0:3F:D5:75:B3:09" SoftName="南京未来高新技术有限公司" SoftNum="空" Zylb="3">
<Fywj/>
<Gfsj>
<GfsjMx Fl="100" Fyxlb="1" Je="0" Jsjc="分部分项工程费+措施项目费+其他项目费-除税工程设备费" Mc="规费" Qfjs="0" Xh="1"/>
<GfsjMx Fl="2.4" Fyxlb="1.1" Je="0" Jsjc="分部分项工程费+措施项目费+其他项目费-除税工程设备费" Mc="社会保险费" Qfjs="0" Xh="1.1"/>
<GfsjMx Fl="0.42" Fyxlb="1.2" Je="0" Jsjc="分部分项工程费+措施项目费+其他项目费-除税工程设备费" Mc="住房公积金" Qfjs="0" Xh="1.2"/>
<GfsjMx Fl="9" Fyxlb="2" Je="0" Jsjc="分部分项工程费+措施项目费+其他项目费+规费-(甲供材料费+甲供设备费)" Mc="税金" Qfjs="0" Xh="2"/>
<GfsjMx Fl="100" Fyxlb="3" Je="0" Jsjc="" Mc="合计" Qfjs="0" Xh="3"/>
</Gfsj>
<Qdxm>
<QdBt Bz="" Je="0" Mc="C.4电气设备安装工程" Xh="1" Zgj="0">
<Qdmx Bz="" Clf="0" Dw="m" Fcf="0" Glf="0" Jsgz="按设计图示尺寸以长度计算（含预留长度及附加长度）" Jxf="0" Lr="0" Mc="电缆YJV-4*70+1*35" Qdbm="030408001002" Rgf="0" Sbf="0" Sl="160" Xh="1" Xmtz="1.名称及型号:铜芯电力电缆敷设。&#xD;&#xA;2.规格:YJV-4*70+1*35mm2(国标)。&#xD;&#xA;3.敷设方式:穿管敷设。" Zcf="0" Zgj="0" Zgr="0" Zhdj="0" Zhhj="0"/>
<Qdmx Bz="" Clf="0" Dw="m" Fcf="0" Glf="0" Jsgz="按设计图示尺寸以长度计算（含预留长度及附加长度）" Jxf="0" Lr="0" Mc="电缆YJV-4*25+1*16" Qdbm="030408001004" Rgf="0" Sbf="0" Sl="100" Xh="2" Xmtz="1.名称及型号:铜芯电力电缆敷设。&#xD;&#xA;2.规格:YJV-4*25+1*16mm2(国标)。&#xD;&#xA;3.敷设方式:穿管敷设。" Zcf="0" Zgj="0" Zgr="0" Zhdj="0" Zhhj="0"/>
<Qdmx Bz="" Clf="0" Dw="m" Fcf="0" Glf="0" Jsgz="按设计图示尺寸以长度计算（含预留长度及附加长度）" Jxf="0" Lr="0" Mc="电缆YJV-5*16" Qdbm="030408001006" Rgf="0" Sbf="0" Sl="100" Xh="3" Xmtz="1.名称及型号:铜芯电力电缆敷设。&#xD;&#xA;2.规格:YJV-4*25+1*16mm2(国标)。&#xD;&#xA;3.敷设方式:穿管敷设。" Zcf="0" Zgj="0" Zgr="0" Zhdj="0" Zhhj="0"/>
<Qdmx Bz="" Clf="0" Dw="m" Fcf="0" Glf="0" Jsgz="按设计图示尺寸以长度计算（含预留长度及附加长度）" Jxf="0" Lr="0" Mc="电缆KVV-5*1.5" Qdbm="030408001003" Rgf="0" Sbf="0" Sl="100" Xh="4" Xmtz="1.名称及型号:铜芯电力电缆敷设。&#xD;&#xA;2.规格:KVV-5*1.5mm2(国标)。&#xD;&#xA;3.敷设方式:穿管敷设。" Zcf="0" Zgj="0" Zgr="0" Zhdj="0" Zhhj="0"/>
<Qdmx Bz="" Clf="0" Dw="m" Fcf="0" Glf="0" Jsgz="按设计图示尺寸以长度计算（含预留长度及附加长度）" Jxf="0" Lr="0" Mc="4*4平方潜水泵专用防水电缆" Qdbm="030408001005" Rgf="0" Sbf="0" Sl="30" Xh="5" Xmtz="1.名称及型号:4*4平方潜水泵专用防水电缆敷设。&#xD;&#xA;2.规格:4*4mm2(国标)。&#xD;&#xA;3.敷设方式:穿管敷设。" Zcf="0" Zgj="0" Zgr="0" Zhdj="0" Zhhj="0"/>
<Qdmx Bz="" Clf="0" Dw="m" Fcf="0" Glf="0" Jsgz="按设计图示尺寸以长度计算。" Jxf="0" Lr="0" Mc="配管SC25" Qdbm="030411001002" Rgf="0" Sbf="0" Sl="100" Xh="6" Xmtz="1.名称 电气配管&#xD;&#xA;2.材质 镀锌钢管&#xD;&#xA;3.规格 DN25&#xD;&#xA;4.配置形式 电缆过路保护管埋地敷设" Zcf="0" Zgj="0" Zgr="0" Zhdj="0" Zhhj="0"/>
<Qdmx Bz="" Clf="0" Dw="m" Fcf="0" Glf="0" Jsgz="按设计图示尺寸以长度计算。" Jxf="0" Lr="0" Mc="配管SC32" Qdbm="030411001003" Rgf="0" Sbf="0" Sl="30" Xh="7" Xmtz="1.名称 电气配管&#xD;&#xA;2.材质 镀锌钢管&#xD;&#xA;3.规格 DN32&#xD;&#xA;4.配置形式 电缆过路保护管埋地敷设" Zcf="0" Zgj="0" Zgr="0" Zhdj="0" Zhhj="0"/>
<Qdmx Bz="" Clf="0" Dw="m" Fcf="0" Glf="0" Jsgz="按设计图示尺寸以长度计算。" Jxf="0" Lr="0" Mc="配管SC100" Qdbm="030411001001" Rgf="0" Sbf="0" Sl="380" Xh="8" Xmtz="1.名称 电气配管&#xD;&#xA;2.材质 镀锌钢管&#xD;&#xA;3.规格 DN100&#xD;&#xA;4.配置形式 电缆过路保护管埋地敷设" Zcf="0" Zgj="0" Zgr="0" Zhdj="0" Zhhj="0"/>
<Qdmx Bz="" Clf="0" Dw="个" Fcf="0" Glf="0" Jsgz="按设计图示数量计算" Jxf="0" Lr="0" Mc="电力电缆头" Qdbm="030408006001" Rgf="0" Sbf="0" Sl="4" Xh="9" Xmtz="1.名称:电力电缆头YJV4*70+1*35" Zcf="0" Zgj="0" Zgr="0" Zhdj="0" Zhhj="0"/>
<Qdmx Bz="" Clf="0" Dw="个" Fcf="0" Glf="0" Jsgz="按设计图示数量计算" Jxf="0" Lr="0" Mc="电力电缆头" Qdbm="030408006002" Rgf="0" Sbf="0" Sl="4" Xh="10" Xmtz="1.名称:电力电缆头YJV4*25+1*16" Zcf="0" Zgj="0" Zgr="0" Zhdj="0" Zhhj="0"/>
<Qdmx Bz="" Clf="0" Dw="台" Fcf="0" Glf="0" Jsgz="按设计图示数量计算" Jxf="0" Lr="0" Mc="室外水泵配电箱AP" Qdbm="030404017001" Rgf="0" Sbf="0" Sl="1" Xh="11" Xmtz="1.名称 落地式配电箱&#xD;&#xA;2.型号 详见选型（配套2个不锈钢立柱）&#xD;&#xA;3.规格 成品单台系统配置，基础混凝土浇筑，详见电气施工图中的系统配置，箱内按规定配线及配置。" Zcf="0" Zgj="0" Zgr="0" Zhdj="0" Zhhj="0"/>
<Qdmx Bz="" Clf="0" Dw="根" Fcf="0" Glf="0" Jsgz="按设计图示数量计算" Jxf="0" Lr="0" Mc="接地极" Qdbm="030409001001" Rgf="0" Sbf="0" Sl="6" Xh="12" Xmtz="1.名称 接地极&#xD;&#xA;2.材质 热镀锌圆钢&#xD;&#xA;3.规格 Φ18 L2500&#xD;&#xA;4.接地形式 按设计要求" Zcf="0" Zgj="0" Zgr="0" Zhdj="0" Zhhj="0"/>
<Qdmx Bz="" Clf="0" Dw="m" Fcf="0" Glf="0" Jsgz="按设计图示尺寸以长度计算（含附加长度）" Jxf="0" Lr="0" Mc="接地母线" Qdbm="030409002001" Rgf="0" Sbf="0" Sl="30" Xh="13" Xmtz="1.名称:户外接地母线敷设&#xD;&#xA;2.材质:热镀锌扁钢&#xD;&#xA;3.规格:-25*4&#xD;&#xA;4.安装形式:焊接" Zcf="0" Zgj="0" Zgr="0" Zhdj="0" Zhhj="0"/>
</QdBt>
<QdBt Bz="" Je="0" Mc="A.1水平防渗工程（安装）" Xh="2" Zgj="0">
<Qdmx Bz="" Clf="0" Dw="台" Fcf="0" Glf="0" Jsgz="按设计图示数量计算" Jxf="0" Lr="0" Mc="地下水导排泵" Qdbm="030109012001" Rgf="0" Sbf="0" Sl="2" Xh="14" Xmtz="1.名称 地下水导排泵（带控制柜一控二）&#xD;&#xA;2.型号 格兰富SEV.65.65.40.2.51D - 96047729&#xD;&#xA;3.规格  Q=20m³/h，H=20m，P=2.2kw&#xD;&#xA;" Zcf="0" Zgj="0" Zgr="0" Zhdj="0" Zhhj="0"/>
<Qdmx Bz="" Clf="0" Dw="座" Fcf="0" Glf="0" Jsgz="按设计图示数量计算" Jxf="0" Lr="0" Mc="阀门井" Qdbm="040504001001" Rgf="0" Sbf="0" Sl="1" Xh="15" Xmtz="1.砌筑材料品种、规格、强度等级 砖砌1.6*2.1*2.1m，阀门井，具体做法及详见图纸&#xD;&#xA;2.盖板材质、规格 玻璃钢盖板&#xD;&#xA;" Zcf="0" Zgj="0" Zgr="0" Zhdj="0" Zhhj="0"/>
<Qdmx Bz="" Clf="0" Dw="个" Fcf="0" Glf="0" Jsgz="按设计图示数量计算" Jxf="0" Lr="0" Mc="止回阀" Qdbm="031003001001" Rgf="0" Sbf="0" Sl="1" Xh="16" Xmtz="1.类型 止回阀&#xD;&#xA;2.材质 PVC&#xD;&#xA;3.规格 DN80" Zcf="0" Zgj="0" Zgr="0" Zhdj="0" Zhhj="0"/>
<Qdmx Bz="" Clf="0" Dw="个" Fcf="0" Glf="0" Jsgz="按设计图示数量计算" Jxf="0" Lr="0" Mc="闸阀" Qdbm="031003001002" Rgf="0" Sbf="0" Sl="2" Xh="17" Xmtz="1.类型 闸阀&#xD;&#xA;2.材质 PVC&#xD;&#xA;3.规格 DN80" Zcf="0" Zgj="0" Zgr="0" Zhdj="0" Zhhj="0"/>
<Qdmx Bz="" Clf="0" Dw="个" Fcf="0" Glf="0" Jsgz="按设计图示数量计算" Jxf="0" Lr="0" Mc="90弯头" Qdbm="031003001003" Rgf="0" Sbf="0" Sl="2" Xh="18" Xmtz="1.类型 90弯头&#xD;&#xA;2.材质 HDPE&#xD;&#xA;3.规格 De90 SDR21" Zcf="0" Zgj="0" Zgr="0" Zhdj="0" Zhhj="0"/>
</QdBt>
<QdBt Bz="" Je="0" Mc="A.1渗沥液导排工程（安装）" Xh="3" Zgj="0">
<Qdmx Bz="" Clf="0" Dw="台" Fcf="0" Glf="0" Jsgz="按设计图示数量计算" Jxf="0" Lr="0" Mc="渗沥液导排泵" Qdbm="030109012002" Rgf="0" Sbf="0" Sl="4" Xh="19" Xmtz="1.名称 渗沥液导排泵	（带控制柜一控二）&#xD;&#xA;2.型号 格兰富SEV.80.80.92.2.51D - 96047207&#xD;&#xA;3.规格  Q=30m³/h，H=30m，P=7.5kw&#xD;&#xA;" Zcf="0" Zgj="0" Zgr="0" Zhdj="0" Zhhj="0"/>
<Qdmx Bz="" Clf="0" Dw="座" Fcf="0" Glf="0" Jsgz="按设计图示数量计算" Jxf="0" Lr="0" Mc="阀门井" Qdbm="040504001002" Rgf="0" Sbf="0" Sl="1" Xh="20" Xmtz="1.砌筑材料品种、规格、强度等级 砖砌0.8*1.2*1.1m，阀门井，具体做法及详见图纸&#xD;&#xA;2.盖板材质、规格 玻璃钢盖板" Zcf="0" Zgj="0" Zgr="0" Zhdj="0" Zhhj="0"/>
<Qdmx Bz="" Clf="0" Dw="座" Fcf="0" Glf="0" Jsgz="按设计图示数量计算" Jxf="0" Lr="0" Mc="计量井" Qdbm="040504001003" Rgf="0" Sbf="0" Sl="1" Xh="21" Xmtz="1.砌筑材料品种、规格、强度等级 砖砌0.8*1.5*1.1m，计量井，具体做法及详见图纸&#xD;&#xA;2.盖板材质、规格 玻璃钢盖板" Zcf="0" Zgj="0" Zgr="0" Zhdj="0" Zhhj="0"/>
<Qdmx Bz="" Clf="0" Dw="个" Fcf="0" Glf="0" Jsgz="按设计图示数量计算" Jxf="0" Lr="0" Mc="止回阀" Qdbm="031003001004" Rgf="0" Sbf="0" Sl="2" Xh="22" Xmtz="1.类型 止回阀&#xD;&#xA;2.材质 PVC&#xD;&#xA;3.规格 DN80" Zcf="0" Zgj="0" Zgr="0" Zhdj="0" Zhhj="0"/>
<Qdmx Bz="" Clf="0" Dw="个" Fcf="0" Glf="0" Jsgz="按设计图示数量计算" Jxf="0" Lr="0" Mc="闸阀" Qdbm="031003001005" Rgf="0" Sbf="0" Sl="4" Xh="23" Xmtz="1.类型 闸阀&#xD;&#xA;2.材质 PVC&#xD;&#xA;3.规格 DN80" Zcf="0" Zgj="0" Zgr="0" Zhdj="0" Zhhj="0"/>
<Qdmx Bz="" Clf="0" Dw="个" Fcf="0" Glf="0" Jsgz="按设计图示数量计算" Jxf="0" Lr="0" Mc="90弯头" Qdbm="031003001006" Rgf="0" Sbf="0" Sl="4" Xh="24" Xmtz="1.类型 90弯头&#xD;&#xA;2.材质 HDPE&#xD;&#xA;3.规格 De90 SDR21" Zcf="0" Zgj="0" Zgr="0" Zhdj="0" Zhhj="0"/>
<Qdmx Bz="" Clf="0" Dw="个" Fcf="0" Glf="0" Jsgz="按设计图示数量计算" Jxf="0" Lr="0" Mc="45弯头" Qdbm="031003001007" Rgf="0" Sbf="0" Sl="4" Xh="25" Xmtz="1.类型 45弯头&#xD;&#xA;2.材质 HDPE&#xD;&#xA;3.规格 De90 SDR21" Zcf="0" Zgj="0" Zgr="0" Zhdj="0" Zhhj="0"/>
<Qdmx Bz="" Clf="0" Dw="个" Fcf="0" Glf="0" Jsgz="按设计图示数量计算" Jxf="0" Lr="0" Mc="三通" Qdbm="031003001008" Rgf="0" Sbf="0" Sl="2" Xh="26" Xmtz="1.类型 三通&#xD;&#xA;2.材质 HDPE&#xD;&#xA;3.规格 De90 SDR21" Zcf="0" Zgj="0" Zgr="0" Zhdj="0" Zhhj="0"/>
<Qdmx Bz="" Clf="0" Dw="台" Fcf="0" Glf="0" Jsgz="按设计图示数量计算" Jxf="0" Lr="0" Mc="电磁流量计" Qdbm="030601004001" Rgf="0" Sbf="0" Sl="1" Xh="27" Xmtz="1.名称 电磁流量计（德国科隆）&#xD;&#xA;2.型号 带不锈钢316电极，PTFE内衬&#xD;&#xA;2.规格 DN80" Zcf="0" Zgj="0" Zgr="0" Zhdj="0" Zhhj="0"/>
</QdBt>
<QdBt Bz="" Je="0" Mc="A.1地表水导排工程" Xh="4" Zgj="0">
<Qdmx Bz="" Clf="0" Dw="台" Fcf="0" Glf="0" Jsgz="按设计图示数量计算" Jxf="0" Lr="0" Mc="临时雨水导排泵" Qdbm="030109012003" Rgf="0" Sbf="0" Sl="2" Xh="28" Xmtz="1.名称 临时雨水导排泵（带控制柜一控二）&#xD;&#xA;2.型号 格兰富SEV.80.80.92.2.51D - 96047207&#xD;&#xA;3.规格  Q=50m³/h，H=22m，P=5.5kw&#xD;&#xA;" Zcf="0" Zgj="0" Zgr="0" Zhdj="0" Zhhj="0"/>
</QdBt>
</Qdxm>
<Csxm>
<ZjCs>
<ZjCsMx Bm="031302001001" Fl="100" Je="0" Js="0" Jsjc="" Mc="安全文明施工" Xh="1" Xmlb="1">
<AqwmfMx Fl="1.5" Je="0" Js="0" Jsjc="" Mc="基本费" Xmlb="1.1"/>
<AqwmfMx Fl="0" Je="0" Js="0" Jsjc="" Mc="增加费" Xmlb="1.2"/>
<AqwmfMx Fl="0.21" Je="0" Js="0" Jsjc="" Mc="扬尘污染防治增加费" Xmlb="1.3"/>
</ZjCsMx>
<ZjCsMx Bm="031302002001" Fl="0" Je="0" Js="0" Jsjc="" Mc="夜间施工" Xh="2" Xmlb="0"/>
<ZjCsMx Bm="031302003001" Fl="0" Je="0" Js="0" Jsjc="" Mc="非夜间施工照明" Xh="3" Xmlb="0"/>
<ZjCsMx Bm="031302005001" Fl="0" Je="0" Js="0" Jsjc="" Mc="冬雨季施工" Xh="4" Xmlb="0"/>
<ZjCsMx Bm="031302006001" Fl="0" Je="0" Js="0" Jsjc="" Mc="已完成工程及设备保护" Xh="5" Xmlb="0"/>
<ZjCsMx Bm="031302008001" Fl="0" Je="0" Js="0" Jsjc="" Mc="临时设施" Xh="6" Xmlb="0"/>
<ZjCsMx Bm="031302009001" Fl="0" Je="0" Js="0" Jsjc="" Mc="赶工措施" Xh="7" Xmlb="0"/>
<ZjCsMx Bm="031302010001" Fl="0" Je="0" Js="0" Jsjc="" Mc="工程按质论价" Xh="8" Xmlb="2"/>
<ZjCsMx Bm="031302011001" Fl="0" Je="0" Js="0" Jsjc="" Mc="住宅分户验收" Xh="9" Xmlb="0"/>
<ZjCsMx Bm="031302012001" Fl="0" Je="0" Js="0" Jsjc="" Mc="建筑工人实名制费用" Xh="10" Xmlb="0"/>
</ZjCs>
<DjCs/>
</Csxm>
<Qtxm>
<QtxmMx Bz="明细详见表-12-1" Je="0" Mc="暂列金额" Xh="1" Xmlb="1"/>
<QtxmMx Bz="" Je="0" Mc="暂估价" Xh="2" Xmlb="2"/>
<QtxmMx Bz="明细详见表-12-2" Je="0" Mc="材料(工程设备)暂估价" Xh="2.1" Xmlb="2.1"/>
<QtxmMx Bz="明细详见表-12-3" Je="0" Mc="专业工程暂估价" Xh="2.2" Xmlb="2.2"/>
<QtxmMx Bz="明细详见表-12-4" Je="0" Mc="计日工" Xh="3" Xmlb="3"/>
<QtxmMx Bz="明细详见表-12-5" Je="0" Mc="总承包服务费" Xh="4" Xmlb="4"/>
</Qtxm>
<Zlje/>
<Clzg/>
<Zygczg/>
<Jrg>
<JrgBt Je="0" Lb="1" Mc="人工" Xh="1"/>
<JrgBt Je="0" Lb="2" Mc="材料" Xh="2"/>
<JrgBt Je="0" Lb="3" Mc="施工机械" Xh="3"/>
<JrgBt Je="0" Lb="4" Mc="企业管理费和利润" Xh="4"/>
</Jrg>
<Zcbfwf/>
<Zjxmjdkzffj/>
<Fbrgycl/>
<Cbrgycl/>
<Rcjhz/>
</Dwgcxx>
</Dxgcxx>
</JingJiBiao>
